SCI-200 CF-B

	SECTION 1. IDENTIFICATION

	Product identifier
	SCI-200 CF-B

	Other Means of Identification
	N. A

	Recommended Use
	Polyurethane adhesive

	Restrictions on Use
	Unknown

	Supplier Identifier
	SCI COATINGS INC.
2821 Boulevard Le Corbusier Laval, Québec
Canada H7L 4J5
Web: www.scicoatings.com

	Emergency Phone No.
	24-Hour Emergency Telephone Number Canada (CANUTEC): (613) 996-6666



	SECTION 2. HAZARD IDENTIFICATION

	Classification
	Flammable liquid Category 3 Carcinogen Category 1B Aspiration Hazard Category 1
Serious eye damage/eye irritation Category 2A Skin Sensitization Category 1

	Label Elements

[image: ]
Signal Word
Danger

Hazard Statements
H226: Flammable liquid and vapour.
H304: May be fatal if swallowed and enters airways. H319: Causes serious eye irritation.
H317: May cause an allergic skin reaction. H351: Suspected of causing cancer.

Precautionary statements
Prevention:
P201 Obtain special instructions before use. P202 Do not handle until all safety precautions have been read and understood. P210 Keep away from heat/sparks/open flames/ hot surfaces. No smoking. P233 Keep container tightly closed. P240 Ground/bond container and receiving equipment. P241 Use explosion proof electrical/ventilating/lighting equipment. P242 Use only non-sparking tools. P243 Take action to prevent static discharge. P280 Wear protective gloves/protective clothing/eye protection/face protection. P261 Avoid breathing dust/fume/gas/mist/vapors/spray. P264 Wash hands thoroughly after handling. P272
Contaminated work clothing must not be allowed out of the workplace. P301 + P310 IF
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	SWALLOWED: Immediately call a POISON CENTER/doctor. P331 Do NOT induce vomiting. P305 + P351 + P338 IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. P337 + P313 If eye irritation persists: Get medical advice/attention. P303 + P361 + P353 IF ON SKIN (or hair): Take off immediately all contaminated clothing. Rinse skin with water/shower. P333 + P313 If skin irritation or rash occurs: Get medical advice/attention. P308 + P313 If exposed or concerned: Get medical advice/attention. P362 + P364 Take off contaminated clothing and wash before reuse. P370 + P378 In case of fire: Use foam, dry chemical, water spray or carbon dioxide (CO2) to extinguish P403 + P235 Store in a well-ventilated place. Keep cool. P405 Store locked up. P501 Dispose of contents/container into safe container in accordance with local,
regional or national regulations.

	Other Hazards:
	Unknown



	Chemical Name
	CAS No.
	% concentration

	Light aromatic solvent naphtha,
petroleum
	64742-95-6
	20-30 %

	Diphenylmethanediisocyanate polymeric
	9016-87-9
	35-50

	4,4’-methylenediphenyl diisocyanate
	101-68-8
	20-35



	SECTION 4. FIRST-AID MEASURES

	First-aid Measures Inhalation:
IF INHALED: Remove from further exposure. For those providing assistance, avoid exposure to yourself or others. Use adequate respiratory protection. If respiratory irritation, dizziness, nausea, or unconsciousness occurs, seek immediate medical assistance. If breathing has stopped, assist ventilation with a mechanical device or use mouth-to mouth resuscitation.
Skin Contact:
Flush with soap and water for a minimum of 15 minutes. Consult a physician if irritation persists or you feel unwell.
Eye Contact:
Rinse immediately with plenty of water for at least 15 minutes. Consult a physician.
Ingestion:
Rinse mouth and then drink plenty of water. Do not induce vomiting. Never induce vomiting or give anything by mouth if the victim is unconscious or having convulsions. Immediate medical attention required.

	Most Important Symptoms and Effects, Acute and Delayed If inhaled:
May cause allergy or asthma symptoms or breathing difficulties if inhaled.
If on skin:
Harmful if in contact with the skin. Causes skin irritation. Exposure may produce an allergic reaction
If in eyes:
Causes serious eye damage.
If Ingested:
Ingestion is likely to be harmful or have adverse effects

	Immediate Medical Attention and Special Treatment: 




	If a physician or medical attention is required, have product container or label at hand.



	SECTION 5. FIRE-FIGHTING MEASURES

	Extinguishing Media Suitable Extinguishing Media
In case of fire: water fog, foam, dry chemical powder, carbon dioxide (CO2)
Unsuitable Extinguishing Media
Do not use water jet as it might spread flame.

	Specific Hazards Arising from the Product
During fire, nitrous gases, fumes/smoke, isocyanates and vapour may be formed. Combustion products may include: acidic hydrogen chloride & hydrogen fluoride, carbon
oxide, hydrocarbons, nitrogen oxides and smoke.

	Special Protective Equipment and Precautions for Fire-fighters
Flammable. Evacuate area. If a leak or spill has not ignited, use water spray to disperse the vapors and to protect personnel attempting to stop a leak. Prevent runoff from fire control or dilution from entering streams, sewers, or drinking water supply. Use water spray to cool fire exposed surfaces and to protect personnel. Self-contained breathing
apparatus and turn-out gear must be worn in case of fire.



	SECTION 6. ACCIDENTAL RELEASE MEASURES

	Personal Precautions, Protective Equipment, and Emergency Procedures
As a general precaution, take personal precaution not to breath gas, vapors, or dusts. Do not get in eyes, on skin or clothing.
Use appropriate personal protection equipment. In the event of an emergency, evacuate any unnecessary personnel.
As an environmental precaution, prevent spillage to sewers, public waters, and do not penetrate ground/soil.

	Methods and Materials for Containment and Clean up
For containment, ensure adequate ventilation and absorb any spill with inert liquid binding material and dispose of waste safely.



	SECTION 7. HANDLING AND STORAGE

	Precautions for Safe Handling
Handle in accordance to good industrial hygiene and safety procedures. Wear respiratory protection when handling. Avoid body contact of containers or contents unless wearing appropriate personal protective equipment. Wear respiratory protection
when handling. Avoid release into the environment.

	Conditions for Safe Storage
Store in cool dry and well-ventilated place. Keep stored in accordance with local, regional, national, and international regulations. Store away from incapable materials.










	SECTION 8. EXPOSURE CONTROLS / PERSONAL PROTECTION

	Control Parameters

	All protective clothing should be appropriately clean and available to dress into before work. The engineering measures or controls and PPE recommendations are only guidelines and may not apply to every situation.
Data not available. For additional information, please consult the corresponding requirements under http://www.ccohs.ca/topics/hazards/chemical/chemicals/

ACGIH® TLV®
OSHA PEL
AIHA® WEEL®
Chemical Name
TWA
STEL [C]
TWA
Ceiling
8-hr TWA
Short-term



























Appropriate Engineering Controls
Local exhaust ventilation required. Make up air should be supplied to balance air that is removed by local or general exhaust ventilation. Provide sufficient ventilation to keep vapors below permissible exposure limit. Emergency eye wash fountains and safety showers should be available in the immediate vicinity of any potential exposure. Ensure all national / local regulations are observed.
Individual Protection Measures
[image: ] [image: ] 
General Measures
Do not eat, drink or smoke during work. Avoid all contact with skin or eye. If clothing comes into contact with material, do not allow out of the workplace. Clean hands and any exposed skin thoroughly after work and before breaks.
Eye / Face Protection
Use tightly sealed goggles or safety glasses with side shields which are resistant to Chemicals.
Skin Protection
Wear chemical resistant protection gloves. Wear impervious clothing as necessary to protect against coming in contact with product.
Respiratory Protection
If insufficient ventilation, wear respiratory protection.



	SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES

	Appearance
	Dark amber Liquid

	Odor
	Not available

	Odor threshold
	Not available

	pH
	Not available

	Melting Point
	Not available

	Initial Boiling Point / Range
	N. A

	Flash point
	N. A

	Evaporation rate
	Not available

	Flammability(solid; gas)
	Not available

	Lower flammable/explosive limit
	Not available

	Upper flammable/explosive limit
	Not available

	Vapor pressure
	Not available

	Vapor density
	Not available

	Specific gravity
	1.13

	Solubility
	Insoluble

	Partition coefficient – n- Octanol/water
	Not available

	Auto-ignition temperature
	Not available

	Decomposition temperature
	Not available

	Viscosity
	Not available



	SECTION 10. STABILITY AND REACTIVITY

	Reactivity
	Non-reactive

	Chemical stability
	Stable under recommended handling and storage conditions

	Possibility of Hazardous reactions
	Risk of bursting. Reacts with alcohols. Reacts with acids. Reacts with
alkalies. Reacts with amines. Risk of exothermic reaction.

	Conditions to avoid
	Keep away from heat, sparks and open flame. Avoid high temperatures. Avoid contact with incompatible
materials.

	Incompatible materials
	Water, amines, substances that react to polyurea

	Hazardous decomposition products
	unknown






	SECTION 11. TOXICOLOGY INFORMATION

	Likely Routes of Administration
Inhalation, skin contact, eye contact, ingestion.
Acute Toxicity
Oral: Harmful if swallowed.
Dermal: Harmful in contact with skin.
LD50 and LC50 Data
Not available
Skin Corrosion/Irritation
Causes skin irritation.
Serious Eye Damage/ Irritation
Causes serious eye damage
STOT (Specific Target Organ Toxicity) – Single Exposure Inhalation May cause allergy or asthma symptoms or breathing difficulties if inhaled. Aspiration Hazard
Not classified based on available data.
STOT(Specific Target Organ Toxicity) – Repeated Exposure Skin, eyes, central nervous system, respiratory system Respiratory and/or Skin Sensitization
May irritate mucous membranes, eyes, nose, and respiratory passages. May cause
asthma attack to persons with pre-existing bronchial hyper reactivity. Exposure to high concentrations may lead to bronchitis, bronchial spasm and pulmonary oedema.




Effects are usually reversible. May cause C.N.S. depression with symptoms of nausea, light-headedness, drowsiness, dizziness, loss of coordination Carcinogenicity
Unknown
Reproductive Toxicity
Not available
Germ Cell Mutagenicity
Not available Interactive Effects Not available





	Chemical Name
	IARC
	ACGIH®
	NTP
	OSHA

	
	
	
	
	

	
	
	
	
	












	SECTION 12. ECOLOGICAL INFORMATION

	Non-hazardous to aquatic environment. This is not required by WHMIS
This is not required by OSHA HCS 2012



	SECTION 13. DISPOSAL CONSIDERATIONS

	Disposal Methods
Dispose of waste material in accordance with all local, regional, national, provincial, territorial and international regulations.



	SECTION 14. TRANSPORT INFORMATION

	

	UN Number; Proper shipping name; Class(es); Packing group (PG) of the IATA (air): UN1263; PAINT RELATED MATERIAL; CLASS 3; PG III



	SECTION 15. REGULATORY INFORMATION

	Not required under Canadian Regulations.








	SECTION 16. OTHER INFORMATION

	Date of Preparation
	August 2020

	Date of Last Revision
	January 4, 2023

	Revision Indicators
	The entire MDSD was change in August 2020 to be in accordance with the WHMIS 2015 which incorporates the Globally Harmonized System of Classification and Labeling
of Chemicals for Canadian Workplaces.



	References
	1. CHOHS Fact Sheets September 2016 ©CCOHS 2016
2. Supplier’s Material Safety Data Sheet(s)




Notice: The facts stated and the recommendations made with respect to the use of this product are based on liable information. No guarantee of accuracy is made. Before using, determine the suitability of the product`s intended use. The purchaser assumes all risks and liability for losses, damage, or expenses, directly or indirectly, arising from the handling or use of the product or from any other cause. All recommendations are made on condition that SCI Coatings Inc will not be liable for any damages resulting from its use since SCI Coatings Inc cannot control the conditions under which the product will be transported, stored, handled or used by the purchaser.
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